|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| # |  |  |  |  |
|  | TechGear 3 Feet USB 2.0 to RS485 Serial Converter Adapter for WinXP/7, Mac USB Cable  (White, Black) |  |  |  |
|  | HE Retail Educational Electronic Hobby Kit | 1. Larger breadboard for complex circuits 2. Multimeter for test and measurement 3. 60+ projects in a illustrated full color eBook 4. All electronic components are provided with the kit 5. No soldering required 6. Practical and presentable projects 7. Includes eBook & videos in DVD 8. 4.8-6V AA battery operated 9. 156+ components included |  |  |
|  | RR Enterprizes Solar and Fuel Cell Electronic Hobby Kit | he 21 snap parts together (no tools required) to build six different working models including an airboat, windmill, puppy, car and two different aeroplanes. |  |  |
|  | Electrobot Electronic Components Electronic Hobby Kit | Breadboard - 1 Pcs • 2 metre hookup wire • Assorted Resistor - 50 Pcs • Assorted Ceramic Capacitor - 50 Pcs • Assorted Capacitor - 70 Pcs • Assorted Transistor - 40 Pcs • Assorted 5mm LED - 50 Pcs • Assorted Diodes - 20 Pcs • Misc Components Assorted Resistor(5 pcs Each) 1 Ohm, 10 Ohm, 100 Ohm, 150 Ohm, 220 Ohm, 1K, 10K, 100K, 150k, 220k, 1M Assorted Ceramic Capacitor(10 Pcs Each) 10 Pf, 100 pf, 102 pf,103 pf, 104 pf Assorted Transistors 547 - 10 pcs, 557 - 10 pcs, KN2222 - 10 pcs, 2N3904 - 5 Pcs, 2N3906 - 5 Pcs Assorted Capacitor 1uf -10 Pcs, 2.2uf-10 Pcs, 4.7uf-10 Pcs, 47uf-10 Pcs, 100uf-10 Pcs,220uf-5 Pcs, 470uf-5 Pcs Assorted 5MM LED (10 Pcs Each) Red, Blue, Green, Yellow, Infrared Diodes (10 Pcs Each) 4007, 4148 Miscellaneous Components 5.1V Zener-2 Pcs, 555 Timer IC, 741 Opamp IC, 4017 Counter IC, 100 Ohm Trimpot, 1K Ohm Trimpot, 5K Ohm Trimpot, 10K Ohm Trimpot, LM317 Voltage Regulator, 7805 Voltage Regulator, 7812 Voltage Regulator, LDR, B20 Buzzer Thermistor -3 Value, 9V Battery, 9V Battery Clip, push buttons-2 Pcs, Condenser mic |  |  |
|  | Robocraze Bread Board Power Supply(3.3V/5V/12V)  (Multicolor) |  |  |  |
|  | EXCELLENT 12V 2A Power Adaptor, Power Supply Ac Input 100-240V Dc Output 12Volt 2Amps Worldwide Adaptor  (Black) | Short Circuit, Over Voltage and Over Current Protection |  |  |
|  | Robosoft Labs AVR ATMEGA16/32 40PIN Development Board with ATMEGA16 , MAX232 , RTC , AT24C32 , ULN2003 IC AND USBASP PROGRAMMER  (Multicolor) | AVR ATMEGA16/32 40PIN Development Board: With this board you can develop and prototype with ATMEGA16/ATMEGA32 (40 pin) microcontrollers. The RS232 driver on board allows easy connection with PC or other embedded hardware. The board have User buttons and status LEDs. The bridge rectifier allow this board to be powered with both AC and DC power supply adapters. FEATURES AVR Development Board for Atmel ATMEGA16/32 ISP Socket for Flashing On board Regulated Power Supply 5v,12v supplies Easy to test with Burg Connecters wires An RS232 Serial Port 7Seg Mulitplexed Display DC Power Supply Connector(12v Ac or Dc) READY INTERFACE For LCD display 16x2 Character 24Cxx (I2C) (EEPROM) RTC (DS1307) 4 LED array Matrix Key Pad 4 Interrupt Switches +12v Relay (one) 8051/8051/AVR USBASP PROGRAMMER Features Flash Burner for AVR Series from ATMEL and 8051/8052 Microcontrollers. Communication - USB Auto Erase before writing and Auto Verify after writing Freeware AVR GCC C Compiler ISP Programming Socket Connects through AVR DUDE USB Powered Device Support AT89s51, AT89s52, AT89s53, AT89s8253 AT90S1200,2313,2323,2343,4414,4433,4434,8515,8535, ATMEGA103,128,1280,1281,16,161,162,163,165,168,169, ATMEGA 2560,2561,32,323,325,3250,329,3290,406,48,64 ATMEGA 640,644,645,6450,649,6490,8,8515,8535,88 ATTINY 11,12,13,15,22,2323,25,26,261,28,44,45,461,84,85,86 AT90CAN128,32,64 - AT90PWM2,3 Package Content AVR ATMEGA16/32 40PIN Development Board with ATMEGA16 , MAX232 , RTC , AT24C32 , ULN2003 IC's 8051/8052/AVR USBASP PROGRAMMER FREE USB CABLE FREE 6 Burg Cable Female 2 Female Programmer Driver (will be sent through Email) Programming Software For AVR (will be sent through Email) |  |  |
|  | TechWiz Educational Electronic Hobby Kit | * (ATmega8A + ATmega328) with base - 1 Piece |  |  |
|  | graylogix Interconnect Electronic Hobby Kit | * USB to Serial/UART or Vise Versa Converter Powered by SiLabs CP2102 Self Powered thru USB 9Pin D type male Connector For Rs232 O/p & TTL Interface |  |  |
|  | Robocraze Raspberry Pi 3 Model B+ Motherboard (New Launch)  (Green) | * The new product is built around BCM2837B0, an updated version of the 64-bit Broadcom application processor used in Raspberry Pi 3B, which incorporates power integrity optimisations, and a heat spreader (that's the shiny metal bit you can see in the photos). Together these allow us to reach higher clock frequencies (or to run at lower voltages to reduce power consumption), and to more accurately monitor and control the temperature of the chip. Dual-band wireless LAN and Bluetooth are provided by the Cypress CYW43455 "combo" chip, connected to a Proant PCB antenna similar to the one used on Raspberry Pi Zero W. |  |  |